    PAD Specification File
    ***************************

    PART TYPE:        LFCPNX-100
    Performance Grade:      9_High-Performance_1.0V
    PACKAGE:          LFG672
    Package Status:                     Final          Version 16

    Thu Nov 30 09:29:45 2023

    Pinout by Port Name:
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | Port Name | Pin/Bank | Buffer Type  | Site  | Properties                                                                                                                                                          |
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | LED1      | R5/1     | LVCMOS33_OUT | PR28B | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | LED2      | R4/1     | LVCMOS33_OUT | PR28A | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | LED3      | R8/1     | LVCMOS33_OUT | PR31A | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | LED4      | R9/1     | LVCMOS33_OUT | PR31B | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | TCK       | M5/1     | LVCMOS33_IN  | PR13A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | TDI       | L9/1     | LVCMOS33_IN  | PR8B  | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | TDO       | M8/1     | LVCMOS33_OUT | PR10B | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | TMS       | L7/1     | LVCMOS33_IN  | PR6B  | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | en        | W21/5    | LVCMOS18H_IN | PB12B | DRIVE:NA SLEWRATE:NA GLITCHFILTER:OFF HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS18H DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF   |
    | reset     | N9/1     | LVCMOS33_IN  | PR24A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 1    | 3.3V  |
    | 5    | 1.8V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +----------+-----------------------+------------+--------------+-----------------+----------------------------------------------------------+
    | Pin/Bank | Pin Info              | Preference | Buffer Type  | Site            | Dual Function                                            |
    +----------+-----------------------+------------+--------------+-----------------+----------------------------------------------------------+
    | A8/81    |                       |            |              | SD7_TXDN        |                                                          |
    | A9/81    |                       |            |              | SD7_TXDP        |                                                          |
    | A11/81   |                       |            |              | SD6_TXDN        |                                                          |
    | A12/81   |                       |            |              | SD6_TXDP        |                                                          |
    | A14/81   |                       |            |              | SD5_TXDN        |                                                          |
    | A15/81   |                       |            |              | SD5_TXDP        |                                                          |
    | A17/81   |                       |            |              | SD4_TXDN        |                                                          |
    | A18/81   |                       |            |              | SD4_TXDP        |                                                          |
    | A21/80   |                       |            |              | SD3_TXDN        |                                                          |
    | A22/80   |                       |            |              | SD3_TXDP        |                                                          |
    | A24/80   |                       |            |              | SD2_TXDN        |                                                          |
    | A25/80   |                       |            |              | SD2_TXDP        |                                                          |
    | AA1/2    |     unused, PULL:DOWN |            |              | PR65A           | EIO                                                      |
    | AA2/2    |     unused, PULL:DOWN |            |              | PR64A           | EIO                                                      |
    | AA4/2    |     unused, PULL:DOWN |            |              | PR62B           | EIO                                                      |
    | AA5/3    |     unused, PULL:DOWN |            |              | PB148B          | PCLKC3_2/COMP3IN/BDQ150                                  |
    | AA6/3    |     unused, PULL:DOWN |            |              | PB146B          | ADC_CN14/BDQ150                                          |
    | AA7/3    |     unused, PULL:DOWN |            |              | PB136A          | BDQ138                                                   |
    | AA10/3   |     unused, PULL:DOWN |            |              | PB124B          | BDQ126                                                   |
    | AA11/3   |     unused, PULL:DOWN |            |              | PB120B          | ADC_CN13/BDQ114                                          |
    | AA12/3   |     unused, PULL:DOWN |            |              | PB110A          | VREF3_1/ADC_CP10/BDQ114                                  |
    | AA13/4   |     unused, PULL:DOWN |            |              | PB100A          | PCLKT4_2/ADC_CP7/BDQ102                                  |
    | AA14/4   |     unused, PULL:DOWN |            |              | PB94B           | BDQ90                                                    |
    | AA17/4   |     unused, PULL:DOWN |            |              | PB82A           | BDQ66                                                    |
    | AA18/4   |     unused, PULL:DOWN |            |              | PB60B           | BDQ54                                                    |
    | AA22/5   |     unused, PULL:DOWN |            |              | PB26B           | BDQ30                                                    |
    | AA23/5   |     unused, PULL:DOWN |            |              | PB28A           | BDQ30                                                    |
    | AA24/5   |     unused, PULL:DOWN |            |              | PB28B           | BDQ30                                                    |
    | AB1/2    |     unused, PULL:DOWN |            |              | PR65B           | EIO                                                      |
    | AB2/2    |     unused, PULL:DOWN |            |              | PR67B           | EIO                                                      |
    | AB3/2    |     unused, PULL:DOWN |            |              | PR67A           | EIO                                                      |
    | AB4/3    |     unused, PULL:DOWN |            |              | PB154A          | PCLKT3_3/LRC_GPLL0T_MFGOUT1/ADC_CP15/BDQ150              |
    | AB6/3    |     unused, PULL:DOWN |            |              | PB142A          | BDQ138                                                   |
    | AB7/3    |     unused, PULL:DOWN |            |              | PB134B          | BDQ138                                                   |
    | AB9/3    |     unused, PULL:DOWN |            |              | PB132A          | BDQ126                                                   |
    | AB11/3   |     unused, PULL:DOWN |            |              | PB118A          | PCLKT3_1/COMP2IP/BDQ114                                  |
    | AB12/3   |     unused, PULL:DOWN |            |              | PB110B          | ADC_CN10/BDQ114                                          |
    | AB13/4   |     unused, PULL:DOWN |            |              | PB100B          | PCLKC4_2/ADC_CN7/BDQ102                                  |
    | AB15/4   |     unused, PULL:DOWN |            |              | PB86A           | BDQ90                                                    |
    | AB18/4   |     unused, PULL:DOWN |            |              | PB58B           | PCLKC4_1/BDQ54                                           |
    | AB19/4   |     unused, PULL:DOWN |            |              | PB58A           | PCLKT4_1/BDQ54                                           |
    | AB20/5   |     unused, PULL:DOWN |            |              | PB48B           | VREF5_2/BDQ42                                            |
    | AB22/5   |     unused, PULL:DOWN |            |              | PB26A           | BDQ30                                                    |
    | AB23/5   |     unused, PULL:DOWN |            |              | PB32A           | BDQ30                                                    |
    | AB24/5   |     unused, PULL:DOWN |            |              | PB32B           | BDQ30                                                    |
    | AB25/5   |     unused, PULL:DOWN |            |              | PB34A           | BDQ30                                                    |
    | AB26/5   |     unused, PULL:DOWN |            |              | PB30B           | BDQSN30                                                  |
    | AC4/3    |     unused, PULL:DOWN |            |              | PB154B          | PCLKC3_3/LRC_GPLL0T_MFGOUT2/ADC_CN15/BDQ150              |
    | AC6/3    |     unused, PULL:DOWN |            |              | PB142B          | BDQ138                                                   |
    | AC7/3    |     unused, PULL:DOWN |            |              | PB134A          | BDQ138                                                   |
    | AC9/3    |     unused, PULL:DOWN |            |              | PB132B          | BDQ126                                                   |
    | AC11/3   |     unused, PULL:DOWN |            |              | PB118B          | PCLKC3_1/COMP2IN/BDQ114                                  |
    | AC12/3   |     unused, PULL:DOWN |            |              | PB112A          | PCLKT3_0/ADC_CP4/BDQ114                                  |
    | AC13/4   |     unused, PULL:DOWN |            |              | PB104A          | ADC_CP9/BDQ102                                           |
    | AC15/4   |     unused, PULL:DOWN |            |              | PB86B           | BDQ90                                                    |
    | AC18/4   |     unused, PULL:DOWN |            |              | PB80A           | BDQ66                                                    |
    | AC19/4   |     unused, PULL:DOWN |            |              | PB56B           | BDQ54                                                    |
    | AC20/5   |     unused, PULL:DOWN |            |              | PB48A           | BDQ42                                                    |
    | AC21/5   |     unused, PULL:DOWN |            |              | PB46A           | PCLKT5_3/BDQ42                                           |
    | AC22/5   |     unused, PULL:DOWN |            |              | PB38A           | BDQ42                                                    |
    | AC24/5   |     unused, PULL:DOWN |            |              | PB34B           | BDQ30                                                    |
    | AC25/5   |     unused, PULL:DOWN |            |              | PB36A           | BDQ30                                                    |
    | AC26/5   |     unused, PULL:DOWN |            |              | PB30A           | BDQS30                                                   |
    | AD1/70   |                       |            |              | ADC_DN1         |                                                          |
    | AD3/3    |     unused, PULL:DOWN |            |              | PB156A          | LRC_GPLL0T_IN/ATB_FORCE/BDQ150                           |
    | AD4/3    |     unused, PULL:DOWN |            |              | PB152A          | ADC_CP12/BDQ150                                          |
    | AD5/3    |     unused, PULL:DOWN |            |              | PB144A          | BDQ138                                                   |
    | AD6/3    |     unused, PULL:DOWN |            |              | PB140A          | BDQ138                                                   |
    | AD9/3    |     unused, PULL:DOWN |            |              | PB130A          | BDQ126                                                   |
    | AD10/3   |     unused, PULL:DOWN |            |              | PB128A          | BDQ126                                                   |
    | AD11/3   |     unused, PULL:DOWN |            |              | PB116A          | ADC_CP8/BDQ114                                           |
    | AD12/3   |     unused, PULL:DOWN |            |              | PB112B          | PCLKC3_0/ADC_CN4/BDQ114                                  |
    | AD13/4   |     unused, PULL:DOWN |            |              | PB104B          | ADC_CN9/BDQ102                                           |
    | AD14/4   |     unused, PULL:DOWN |            |              | PB96A           | BDQ90                                                    |
    | AD15/4   |     unused, PULL:DOWN |            |              | PB88A           | BDQ90                                                    |
    | AD18/4   |     unused, PULL:DOWN |            |              | PB80B           | BDQ66                                                    |
    | AD20/4   |     unused, PULL:DOWN |            |              | PB56A           | BDQ54                                                    |
    | AD21/4   |     unused, PULL:DOWN |            |              | PB52A           | PCLKT4_0/BDQ54                                           |
    | AD22/5   |     unused, PULL:DOWN |            |              | PB46B           | PCLKC5_3/BDQ42                                           |
    | AD23/5   |     unused, PULL:DOWN |            |              | PB38B           | BDQ42                                                    |
    | AD25/5   |     unused, PULL:DOWN |            |              | PB40A           | PCLKT5_2/BDQ42                                           |
    | AD26/5   |     unused, PULL:DOWN |            |              | PB36B           | BDQ30                                                    |
    | AE1/70   |                       |            |              | ADC_DP1         |                                                          |
    | AE2/70   |                       |            |              | ADC_DN0         |                                                          |
    | AE3/3    |     unused, PULL:DOWN |            |              | PB156B          | LRC_GPLL0C_IN/VREF3_2/ATB_SENSE/BDQ150                   |
    | AE4/3    |     unused, PULL:DOWN |            |              | PB152B          | ADC_CN12/BDQ150                                          |
    | AE5/3    |     unused, PULL:DOWN |            |              | PB144B          | BDQ138                                                   |
    | AE6/3    |     unused, PULL:DOWN |            |              | PB140B          | BDQ138                                                   |
    | AE9/3    |     unused, PULL:DOWN |            |              | PB130B          | BDQ126                                                   |
    | AE10/3   |     unused, PULL:DOWN |            |              | PB128B          | BDQ126                                                   |
    | AE11/3   |     unused, PULL:DOWN |            |              | PB116B          | ADC_CN8/BDQ114                                           |
    | AE12/4   |     unused, PULL:DOWN |            |              | PB106B          | PCLKC4_3/BDQ102                                          |
    | AE13/4   |     unused, PULL:DOWN |            |              | PB106A          | PCLKT4_3/BDQ102                                          |
    | AE14/4   |     unused, PULL:DOWN |            |              | PB96B           | BDQ90                                                    |
    | AE15/4   |     unused, PULL:DOWN |            |              | PB88B           | BDQ90                                                    |
    | AE19/4   |     unused, PULL:DOWN |            |              | PB64B           | BDQ66                                                    |
    | AE21/4   |     unused, PULL:DOWN |            |              | PB52B           | PCLKC4_0/BDQ54                                           |
    | AE22/4   |     unused, PULL:DOWN |            |              | PB50A           | VREF4_1/BDQ54                                            |
    | AE23/4   |     unused, PULL:DOWN |            |              | PB50B           | BDQ54                                                    |
    | AE24/5   |     unused, PULL:DOWN |            |              | PB44A           | BDQ42                                                    |
    | AE25/5   |     unused, PULL:DOWN |            |              | PB40B           | PCLKC5_2/BDQ42                                           |
    | AE26/5   |     unused, PULL:DOWN |            |              | PB42A           | BDQS42                                                   |
    | AF2/70   |                       |            |              | ADC_DP0         |                                                          |
    | AF3/3    |     unused, PULL:DOWN |            |              | PB150B          | ADC_CN11/BDQSN150                                        |
    | AF4/3    |     unused, PULL:DOWN |            |              | PB150A          | ADC_CP11/BDQS150                                         |
    | AF5/3    |     unused, PULL:DOWN |            |              | PB138B          | BDQSN138                                                 |
    | AF6/3    |     unused, PULL:DOWN |            |              | PB138A          | BDQS138                                                  |
    | AF9/3    |     unused, PULL:DOWN |            |              | PB126B          | BDQSN126                                                 |
    | AF10/3   |     unused, PULL:DOWN |            |              | PB126A          | BDQS126                                                  |
    | AF11/3   |     unused, PULL:DOWN |            |              | PB114B          | COMP1IN/BDQSN114                                         |
    | AF12/3   |     unused, PULL:DOWN |            |              | PB114A          | COMP1IP/BDQS114                                          |
    | AF13/4   |     unused, PULL:DOWN |            |              | PB102B          | ADC_CN6/BDQSN102                                         |
    | AF14/4   |     unused, PULL:DOWN |            |              | PB102A          | ADC_CP6/BDQS102                                          |
    | AF15/4   |     unused, PULL:DOWN |            |              | PB90A           | BDQS90                                                   |
    | AF16/4   |     unused, PULL:DOWN |            |              | PB90B           | BDQSN90                                                  |
    | AF19/4   |     unused, PULL:DOWN |            |              | PB64A           | BDQ66                                                    |
    | AF20/4   |     unused, PULL:DOWN |            |              | PB66B           | BDQSN66                                                  |
    | AF21/4   |     unused, PULL:DOWN |            |              | PB66A           | BDQS66                                                   |
    | AF22/4   |     unused, PULL:DOWN |            |              | PB54A           | BDQS54                                                   |
    | AF23/4   |     unused, PULL:DOWN |            |              | PB54B           | BDQSN54                                                  |
    | AF24/5   |     unused, PULL:DOWN |            |              | PB44B           | BDQ42                                                    |
    | AF25/5   |     unused, PULL:DOWN |            |              | PB42B           | BDQSN42                                                  |
    | B10/81   |                       |            |              | SD7_RXDP        |                                                          |
    | B13/81   |                       |            |              | SD6_RXDP        |                                                          |
    | B16/81   |                       |            |              | SD5_RXDN        |                                                          |
    | B19/81   |                       |            |              | SD4_RXDN        |                                                          |
    | B20/81   |                       |            |              | SD4_RXDP        |                                                          |
    | B23/80   |                       |            |              | SD2_RXDN        |                                                          |
    | B26/80   |                       |            |              | SD1_TXDN        |                                                          |
    | C10/81   |                       |            |              | SD7_RXDN        |                                                          |
    | C12/81   |                       |            |              | SD6_RXDN        |                                                          |
    | C14/81   |                       |            |              | SDQ1_REFCLKP    |                                                          |
    | C16/81   |                       |            |              | SD5_RXDP        |                                                          |
    | C18/80   |                       |            |              | SD3_REXT        |                                                          |
    | C21/80   |                       |            |              | SD3_RXDP        |                                                          |
    | C22/80   |                       |            |              | SD3_RXDN        |                                                          |
    | C24/80   |                       |            |              | SD2_RXDP        |                                                          |
    | C26/80   |                       |            |              | SD1_TXDP        |                                                          |
    | D9/83    |                       |            |              | SD_EXT1_REFCLKN |                                                          |
    | D11/83   |                       |            |              | SD_EXT0_REFCLKP |                                                          |
    | D13/81   |                       |            |              | SDQ1_REFCLKN    |                                                          |
    | D15/81   |                       |            |              | SD6_REXT        |                                                          |
    | D17/81   |                       |            |              | SD4_REXT        |                                                          |
    | D18/80   |                       |            |              | SD3_REFRET      |                                                          |
    | D19/80   |                       |            |              | SD2_REXT        |                                                          |
    | D25/80   |                       |            |              | SD1_RXDN        |                                                          |
    | E10/83   |                       |            |              | SD_EXT1_REFCLKP |                                                          |
    | E11/83   |                       |            |              | SD_EXT0_REFCLKN |                                                          |
    | E12/81   |                       |            |              | SD7_REFRET      |                                                          |
    | E13/81   |                       |            |              | SD7_REXT        |                                                          |
    | E15/81   |                       |            |              | SD6_REFRET      |                                                          |
    | E17/81   |                       |            |              | SD4_REFRET      |                                                          |
    | E19/80   |                       |            |              | SD2_REFRET      |                                                          |
    | E20/80   |                       |            |              | SDQ0_REFCLKN    |                                                          |
    | E21/80   |                       |            |              | SD0_REXT        |                                                          |
    | E22/80   |                       |            |              | SD0_REFRET      |                                                          |
    | E24/80   |                       |            |              | SD1_RXDP        |                                                          |
    | E26/80   |                       |            |              | SD0_TXDN        |                                                          |
    | F20/80   |                       |            |              | SDQ0_REFCLKP    |                                                          |
    | F26/80   |                       |            |              | SD0_TXDP        |                                                          |
    | G2/0     | Reserved: sysCONFIG   |            |              | PT134A          | INITN                                                    |
    | G4/0     | Reserved: sysCONFIG   |            |              | PT134B          | PROGRAMN                                                 |
    | G5/0     | Reserved: sysCONFIG   |            |              | PT136B          | DONE/S0_OUT                                              |
    | G6/0     |     unused, PULL:DOWN |            |              | PT136A          | MCLK/PCLKT0_0/S0_IN                                      |
    | G7/0     |     unused, PULL:DOWN |            |              | PT138A          | MCSN/S1_IN/PCLKT0_1                                      |
    | G20/80   |                       |            |              | SD1_REXT        |                                                          |
    | G21/80   |                       |            |              | SD1_REFRET      |                                                          |
    | G24/80   |                       |            |              | SD0_RXDP        |                                                          |
    | G25/80   |                       |            |              | SD0_RXDN        |                                                          |
    | H1/0     |     unused, PULL:DOWN |            |              | PT144B          | S7_OUT                                                   |
    | H2/0     |     unused, PULL:DOWN |            |              | PT144A          | S7_IN                                                    |
    | H3/0     |     unused, PULL:DOWN |            |              | PT142B          | MCSNO/MSDO/S6_OUT                                        |
    | H4/0     |     unused, PULL:DOWN |            |              | PT142A          | MD3/SD7/S6_IN/OSC_BURST                                  |
    | H6/0     |     unused, PULL:DOWN |            |              | PT140A          | MISO/MD1/SD5/S2_IN/OSC_HI                                |
    | H7/0     |     unused, PULL:DOWN |            |              | PT138B          | MOSI/MD0/SD4/S1_OUT                                      |
    | H20/7    |     unused, PULL:DOWN |            |              | PL3A            | ULC_GPLL0T_IN/EIO                                        |
    | H21/7    |     unused, PULL:DOWN |            |              | PL3B            | EIO                                                      |
    | H22/7    |     unused, PULL:DOWN |            |              | PL4A            | ULC_GPLL0T_MFGOUT1/EIO                                   |
    | H23/7    |     unused, PULL:DOWN |            |              | PL4B            | ULC_GPLL0T_MFGOUT2/EIO                                   |
    | H26/7    |     unused, PULL:DOWN |            |              | PL6A            | EIO                                                      |
    | J1/0     |     unused, PULL:DOWN |            |              | PT146A          |                                                          |
    | J2/0     |     unused, PULL:DOWN |            |              | PT146B          |                                                          |
    | J3/0     |     unused, PULL:DOWN |            |              | PT148A          |                                                          |
    | J5/0     |     unused, PULL:DOWN |            |              | PT148B          |                                                          |
    | J6/0     |     unused, PULL:DOWN |            |              | PT150A          |                                                          |
    | J7/0     |     unused, PULL:DOWN |            |              | PT150B          |                                                          |
    | J15/81   |                       |            |              | SD5_REFRET      |                                                          |
    | J19/7    |     unused, PULL:DOWN |            |              | PL13A           | EIO                                                      |
    | J20/7    |     unused, PULL:DOWN |            |              | PL11B           | EIO                                                      |
    | J21/7    |     unused, PULL:DOWN |            |              | PL11A           | EIO                                                      |
    | J22/7    |     unused, PULL:DOWN |            |              | PL10B           | EIO                                                      |
    | J23/7    |     unused, PULL:DOWN |            |              | PL10A           | EIO                                                      |
    | J24/7    |     unused, PULL:DOWN |            |              | PL8B            | EIO                                                      |
    | J25/7    |     unused, PULL:DOWN |            |              | PL8A            | EIO                                                      |
    | J26/7    |     unused, PULL:DOWN |            |              | PL6B            | EIO                                                      |
    | K2/0     |     unused, PULL:DOWN |            |              | PT156B          |                                                          |
    | K3/0     |     unused, PULL:DOWN |            |              | PT156A          |                                                          |
    | K4/0     |     unused, PULL:DOWN |            |              | PT154B          |                                                          |
    | K5/0     |     unused, PULL:DOWN |            |              | PT140B          | MD2/SD6/S2_OUT                                           |
    | K6/0     |     unused, PULL:DOWN |            |              | PT154A          |                                                          |
    | K7/0     |     unused, PULL:DOWN |            |              | PT152B          |                                                          |
    | K8/0     |     unused, PULL:DOWN |            |              | PT152A          |                                                          |
    | K15/81   |                       |            |              | SD5_REXT        |                                                          |
    | K18/7    |     unused, PULL:DOWN |            |              | PL15A           | EIO                                                      |
    | K19/7    |     unused, PULL:DOWN |            |              | PL15B           | EIO                                                      |
    | K20/7    |     unused, PULL:DOWN |            |              | PL13B           | EIO                                                      |
    | K21/7    |     unused, PULL:DOWN |            |              | PL17A           | EIO                                                      |
    | K24/7    |     unused, PULL:DOWN |            |              | PL19A           | EIO                                                      |
    | K25/7    |     unused, PULL:DOWN |            |              | PL19B           | EIO                                                      |
    | K26/7    |     unused, PULL:DOWN |            |              | PL20A           | EIO                                                      |
    | L1/1     |     unused, PULL:DOWN |            |              | PR3B            | S8_IN/EIO                                                |
    | L2/1     |     unused, PULL:DOWN |            |              | PR4A            | URC_GPLL0T_IN/S8_OUT/EIO                                 |
    | L3/1     |     unused, PULL:DOWN |            |              | PR4B            | SD10                                                     |
    | L6/1     |     unused, PULL:DOWN |            |              | PR6A            | URC_GPLL0T_MFGOUT1/EIO                                   |
    | L7/1     | TMS                   |            | LVCMOS33_IN  | PR6B            | TMS/SCSN/URC_GPLL0T_MFGOUT2/S5_IN                        |
    | L8/1     |     unused, PULL:DOWN |            |              | PR8A            | EIO                                                      |
    | L9/1     | TDI                   |            | LVCMOS33_IN  | PR8B            | TDI/SSI/SD0/S5_OUT                                       |
    | L19/7    |     unused, PULL:DOWN |            |              | PL26B           | EIO                                                      |
    | L20/7    |     unused, PULL:DOWN |            |              | PL26A           | EIO                                                      |
    | L21/7    |     unused, PULL:DOWN |            |              | PL17B           | EIO                                                      |
    | L22/7    |     unused, PULL:DOWN |            |              | PL24B           | EIO                                                      |
    | L23/7    |     unused, PULL:DOWN |            |              | PL24A           | EIO                                                      |
    | L24/7    |     unused, PULL:DOWN |            |              | PL22B           | EIO                                                      |
    | L25/7    |     unused, PULL:DOWN |            |              | PL22A           | EIO                                                      |
    | L26/7    |     unused, PULL:DOWN |            |              | PL20B           | EIO                                                      |
    | M1/1     |     unused, PULL:DOWN |            |              | PR17A           | SD12                                                     |
    | M2/1     |     unused, PULL:DOWN |            |              | PR15B           | SD8                                                      |
    | M3/1     |     unused, PULL:DOWN |            |              | PR15A           | SD9                                                      |
    | M4/1     |     unused, PULL:DOWN |            |              | PR13B           | PMU_WAKEUPN/SD11/S4_OUT                                  |
    | M5/1     | TCK                   |            | LVCMOS33_IN  | PR13A           | TCK/SCLK/PMU_EXT_CLK                                     |
    | M6/1     |     unused, PULL:DOWN |            |              | PR11A           | SD3/SDA/USER_SDA/S4_IN                                   |
    | M7/1     |     unused, PULL:DOWN |            |              | PR11B           | SD2/SCL/USER_SCL/S3_IN                                   |
    | M8/1     | TDO                   |            | LVCMOS33_OUT | PR10B           | TDO/SSO/SD1/S3_OUT                                       |
    | M9/1     |     unused, PULL:DOWN |            |              | PR10A           | EIO                                                      |
    | M26/7    |     unused, PULL:DOWN |            |              | PL28A           | PCLKT7_2/EIO                                             |
    | N1/1     |     unused, PULL:DOWN |            |              | PR17B           | SD13                                                     |
    | N2/1     |     unused, PULL:DOWN |            |              | PR19A           | SD14                                                     |
    | N3/1     |     unused, PULL:DOWN |            |              | PR19B           | SD15                                                     |
    | N4/1     |     unused, PULL:DOWN |            |              | PR20A           | EIO                                                      |
    | N5/1     |     unused, PULL:DOWN |            |              | PR20B           | EIO                                                      |
    | N6/1     |     unused, PULL:DOWN |            |              | PR22A           | EIO                                                      |
    | N7/1     |     unused, PULL:DOWN |            |              | PR22B           | EIO                                                      |
    | N8/1     |     unused, PULL:DOWN |            |              | PR24B           | EIO                                                      |
    | N9/1     | reset                 | LOCATED    | LVCMOS33_IN  | PR24A           | EIO                                                      |
    | N19/7    |     unused, PULL:DOWN |            |              | PL35A           | EIO                                                      |
    | N20/7    |     unused, PULL:DOWN |            |              | PL33B           | EIO                                                      |
    | N21/7    |     unused, PULL:DOWN |            |              | PL33A           | EIO                                                      |
    | N22/7    |     unused, PULL:DOWN |            |              | PL31B           | EIO                                                      |
    | N23/7    |     unused, PULL:DOWN |            |              | PL31A           | PCLKT7_0/EIO                                             |
    | N24/7    |     unused, PULL:DOWN |            |              | PL29B           | EIO                                                      |
    | N25/7    |     unused, PULL:DOWN |            |              | PL29A           | PCLKT7_1/EIO                                             |
    | N26/7    |     unused, PULL:DOWN |            |              | PL28B           | EIO                                                      |
    | P8/1     |     unused, PULL:DOWN |            |              | PR26B           | EIO                                                      |
    | P9/1     |     unused, PULL:DOWN |            |              | PR26A           | EIO                                                      |
    | P18/7    |     unused, PULL:DOWN |            |              | PL35B           | EIO                                                      |
    | P19/7    |     unused, PULL:DOWN |            |              | PL38A           | EIO                                                      |
    | P20/7    |     unused, PULL:DOWN |            |              | PL38B           | EIO                                                      |
    | P21/6    |     unused, PULL:DOWN |            |              | PL44B           | EIO                                                      |
    | P22/6    |     unused, PULL:DOWN |            |              | PL44A           | PCLKT6_1/EIO                                             |
    | P23/6    |     unused, PULL:DOWN |            |              | PL42B           | EIO                                                      |
    | P24/6    |     unused, PULL:DOWN |            |              | PL42A           | PCLKT6_0/EIO                                             |
    | P25/6    |     unused, PULL:DOWN |            |              | PL40B           | EIO                                                      |
    | P26/6    |     unused, PULL:DOWN |            |              | PL40A           | EIO                                                      |
    | R4/1     | LED2                  | LOCATED    | LVCMOS33_OUT | PR28A           | PCLKT1_2/EIO                                             |
    | R5/1     | LED1                  | LOCATED    | LVCMOS33_OUT | PR28B           | EIO                                                      |
    | R6/1     |     unused, PULL:DOWN |            |              | PR29A           | PCLKT1_1/EIO                                             |
    | R7/1     |     unused, PULL:DOWN |            |              | PR29B           | EIO                                                      |
    | R8/1     | LED3                  | LOCATED    | LVCMOS33_OUT | PR31A           | PCLKT1_0/EIO                                             |
    | R9/1     | LED4                  | LOCATED    | LVCMOS33_OUT | PR31B           | EIO                                                      |
    | R18/6    |     unused, PULL:DOWN |            |              | PL47B           | EIO                                                      |
    | R19/6    |     unused, PULL:DOWN |            |              | PL47A           | EIO                                                      |
    | R20/6    |     unused, PULL:DOWN |            |              | PL46A           | PCLKT6_2/EIO                                             |
    | R21/6    |     unused, PULL:DOWN |            |              | PL46B           | EIO                                                      |
    | R22/6    |     unused, PULL:DOWN |            |              | PL49A           | EIO                                                      |
    | R25/6    |     unused, PULL:DOWN |            |              | PL51A           | EIO                                                      |
    | R26/6    |     unused, PULL:DOWN |            |              | PL51B           | EIO                                                      |
    | T1/2     |     unused, PULL:DOWN |            |              | PR42A           | PCLKT2_0/EIO                                             |
    | T2/2     |     unused, PULL:DOWN |            |              | PR40B           | EIO                                                      |
    | T3/2     |     unused, PULL:DOWN |            |              | PR40A           | EIO                                                      |
    | T4/1     |     unused, PULL:DOWN |            |              | PR38B           | EIO                                                      |
    | T5/1     |     unused, PULL:DOWN |            |              | PR38A           | EIO                                                      |
    | T6/1     |     unused, PULL:DOWN |            |              | PR35B           | EIO                                                      |
    | T7/1     |     unused, PULL:DOWN |            |              | PR35A           | EIO                                                      |
    | T8/1     |     unused, PULL:DOWN |            |              | PR33B           | EIO                                                      |
    | T18/6    |     unused, PULL:DOWN |            |              | PL58B           | EIO                                                      |
    | T19/6    |     unused, PULL:DOWN |            |              | PL58A           | EIO                                                      |
    | T20/6    |     unused, PULL:DOWN |            |              | PL56B           | EIO                                                      |
    | T21/6    |     unused, PULL:DOWN |            |              | PL56A           | EIO                                                      |
    | T22/6    |     unused, PULL:DOWN |            |              | PL49B           | EIO                                                      |
    | T23/6    |     unused, PULL:DOWN |            |              | PL55B           | EIO                                                      |
    | T24/6    |     unused, PULL:DOWN |            |              | PL55A           | EIO                                                      |
    | T25/6    |     unused, PULL:DOWN |            |              | PL53B           | EIO                                                      |
    | T26/6    |     unused, PULL:DOWN |            |              | PL53A           | EIO                                                      |
    | U1/2     |     unused, PULL:DOWN |            |              | PR42B           | EIO                                                      |
    | U2/2     |     unused, PULL:DOWN |            |              | PR44A           | PCLKT2_1/EIO                                             |
    | U3/2     |     unused, PULL:DOWN |            |              | PR44B           | EIO                                                      |
    | U6/2     |     unused, PULL:DOWN |            |              | PR46A           | PCLKT2_2/EIO                                             |
    | U7/2     |     unused, PULL:DOWN |            |              | PR46B           | EIO                                                      |
    | U8/1     |     unused, PULL:DOWN |            |              | PR33A           | EIO                                                      |
    | U18/6    |     unused, PULL:DOWN |            |              | PL60B           | EIO                                                      |
    | U19/6    |     unused, PULL:DOWN |            |              | PL60A           | EIO                                                      |
    | U22/6    |     unused, PULL:DOWN |            |              | PL62A           | EIO                                                      |
    | U23/6    |     unused, PULL:DOWN |            |              | PL62B           | EIO                                                      |
    | U24/6    |     unused, PULL:DOWN |            |              | PL64A           | EIO                                                      |
    | U25/6    |     unused, PULL:DOWN |            |              | PL64B           | EIO                                                      |
    | U26/5    |     unused, PULL:DOWN |            |              | PB6A            | BDQS6                                                    |
    | V1/2     |     unused, PULL:DOWN |            |              | PR49A           | EIO                                                      |
    | V2/2     |     unused, PULL:DOWN |            |              | PR49B           | EIO                                                      |
    | V3/2     |     unused, PULL:DOWN |            |              | PR51A           | EIO                                                      |
    | V4/2     |     unused, PULL:DOWN |            |              | PR51B           | EIO                                                      |
    | V5/2     |     unused, PULL:DOWN |            |              | PR53A           | EIO                                                      |
    | V6/2     |     unused, PULL:DOWN |            |              | PR53B           | EIO                                                      |
    | V7/2     |     unused, PULL:DOWN |            |              | PR47B           | EIO                                                      |
    | V8/2     |     unused, PULL:DOWN |            |              | PR47A           | EIO                                                      |
    | V18/6    |     unused, PULL:DOWN |            |              | PL65A           | EIO                                                      |
    | V19/6    |     unused, PULL:DOWN |            |              | PL65B           | EIO                                                      |
    | V20/6    |     unused, PULL:DOWN |            |              | PL67A           | EIO                                                      |
    | V21/6    |     unused, PULL:DOWN |            |              | PL67B           | EIO                                                      |
    | V22/5    |     unused, PULL:DOWN |            |              | PB4B            | PCLKC5_0/LLC_GPLL0T_MFGOUT2/CDR_RXN1/ADC_CN1/COMP2N/BDQ6 |
    | V23/5    |     unused, PULL:DOWN |            |              | PB4A            | PCLKT5_0/LLC_GPLL0T_MFGOUT1/CDR_RXP1/ADC_CP1/COMP2P/BDQ6 |
    | V24/5    |     unused, PULL:DOWN |            |              | PB2A            | LLC_GPLL0T_IN/CDR_RXP0/VREF5_1/ADC_CP0/COMP1P/BDQ6       |
    | V25/5    |     unused, PULL:DOWN |            |              | PB2B            | LLC_GPLL0C_IN/CDR_RXN0/ADC_CN0/COMP1N/BDQ6               |
    | V26/5    |     unused, PULL:DOWN |            |              | PB6B            | BDQSN6                                                   |
    | W1/2     |     unused, PULL:DOWN |            |              | PR60A           | EIO                                                      |
    | W2/2     |     unused, PULL:DOWN |            |              | PR58B           | EIO                                                      |
    | W3/2     |     unused, PULL:DOWN |            |              | PR58A           | EIO                                                      |
    | W4/2     |     unused, PULL:DOWN |            |              | PR56B           | EIO                                                      |
    | W5/2     |     unused, PULL:DOWN |            |              | PR56A           | EIO                                                      |
    | W6/2     |     unused, PULL:DOWN |            |              | PR55B           | EIO                                                      |
    | W7/2     |     unused, PULL:DOWN |            |              | PR55A           | EIO                                                      |
    | W10/3    |     unused, PULL:DOWN |            |              | PB122B          | BDQ126                                                   |
    | W11/3    |     unused, PULL:DOWN |            |              | PB122A          | BDQ126                                                   |
    | W12/4    |     unused, PULL:DOWN |            |              | PB108B          | VREF4_2/BDQ102                                           |
    | W13/4    |     unused, PULL:DOWN |            |              | PB98A           | ADC_CP5/BDQ102                                           |
    | W14/4    |     unused, PULL:DOWN |            |              | PB92B           | BDQ90                                                    |
    | W15/4    |     unused, PULL:DOWN |            |              | PB92A           | BDQ90                                                    |
    | W16/4    |     unused, PULL:DOWN |            |              | PB84B           | BDQ66                                                    |
    | W17/4    |     unused, PULL:DOWN |            |              | PB62A           | BDQ66                                                    |
    | W18/4    |     unused, PULL:DOWN |            |              | PB62B           | BDQ66                                                    |
    | W21/5    | en                    | LOCATED    | LVCMOS18H_IN | PB12B           | CDR1_TESTN/BDQ6                                          |
    | W22/5    |     unused, PULL:DOWN |            |              | PB12A           | CDR1_TESTP/BDQ6                                          |
    | W23/5    |     unused, PULL:DOWN |            |              | PB10B           | PCLKC5_1/CDR0_TESTN/ADC_CN2/COMP3N/BDQ6                  |
    | W24/5    |     unused, PULL:DOWN |            |              | PB10A           | PCLKT5_1/CDR0_TESTP/ADC_CP2/COMP3P/BDQ6                  |
    | W25/5    |     unused, PULL:DOWN |            |              | PB8A            | ADC_CP3/BDQ6                                             |
    | W26/5    |     unused, PULL:DOWN |            |              | PB8B            | ADC_CN3/BDQ6                                             |
    | Y1/2     |     unused, PULL:DOWN |            |              | PR60B           | EIO                                                      |
    | Y2/2     |     unused, PULL:DOWN |            |              | PR64B           | EIO                                                      |
    | Y4/2     |     unused, PULL:DOWN |            |              | PR62A           | EIO                                                      |
    | Y5/3     |     unused, PULL:DOWN |            |              | PB148A          | PCLKT3_2/COMP3IP/BDQ150                                  |
    | Y6/3     |     unused, PULL:DOWN |            |              | PB146A          | ADC_CP14/BDQ150                                          |
    | Y7/3     |     unused, PULL:DOWN |            |              | PB136B          | BDQ138                                                   |
    | Y10/3    |     unused, PULL:DOWN |            |              | PB124A          | BDQ126                                                   |
    | Y11/3    |     unused, PULL:DOWN |            |              | PB120A          | ADC_CP13/BDQ114                                          |
    | Y12/4    |     unused, PULL:DOWN |            |              | PB108A          | BDQ102                                                   |
    | Y13/4    |     unused, PULL:DOWN |            |              | PB98B           | ADC_CN5/BDQ102                                           |
    | Y14/4    |     unused, PULL:DOWN |            |              | PB94A           | BDQ90                                                    |
    | Y16/4    |     unused, PULL:DOWN |            |              | PB84A           | BDQ66                                                    |
    | Y17/4    |     unused, PULL:DOWN |            |              | PB82B           | BDQ66                                                    |
    | Y18/4    |     unused, PULL:DOWN |            |              | PB60A           | BDQ54                                                    |
    +----------+-----------------------+------------+--------------+-----------------+----------------------------------------------------------+

    sysCONFIG Pins:
    +----------+-----------------------------------+----------+--------------+
    | Pad Name | sysCONFIG Pin Name                | Pin/Bank | Buffer Type  |
    +----------+-----------------------------------+----------+--------------+
    | PT134A   | INITN                             | G2/0     |              |
    | PT134B   | PROGRAMN                          | G4/0     |              |
    | PT136B   | DONE/S0_OUT                       | G5/0     |              |
    | PR13A    | TCK/SCLK/PMU_EXT_CLK              | M5/1     | LVCMOS33_IN  |
    | PR10B    | TDO/SSO/SD1/S3_OUT                | M8/1     | LVCMOS33_OUT |
    | PR8B     | TDI/SSI/SD0/S5_OUT                | L9/1     | LVCMOS33_IN  |
    | PR6B     | TMS/SCSN/URC_GPLL0T_MFGOUT2/S5_IN | L7/1     | LVCMOS33_IN  |
    +----------+-----------------------------------+----------+--------------+

    Locate Constraints for each Pin:

    ldc_set_location -site {R5} [ get_ports {LED1} ]
    ldc_set_location -site {R4} [ get_ports {LED2} ]
    ldc_set_location -site {R8} [ get_ports {LED3} ]
    ldc_set_location -site {R9} [ get_ports {LED4} ]
    ldc_set_location -site {M5} [ get_ports {TCK} ]
    ldc_set_location -site {L9} [ get_ports {TDI} ]
    ldc_set_location -site {M8} [ get_ports {TDO} ]
    ldc_set_location -site {L7} [ get_ports {TMS} ]
    ldc_set_location -site {W21} [ get_ports {en} ]
    ldc_set_location -site {N9} [ get_ports {reset} ]

    Copyright (c) 2002-2022 Lattice Semiconductor Corporation,  All rights reserved.

    Thu Nov 30 09:29:45 2023