                             Lattice Mapping Report File

    Design:  Top
    Family:  LFCPNX
    Device:  LFCPNX-100
    Package: LFG672
    Performance Grade:  9_High-Performance_1.0V

    Mapper:    version Radiant Software (64-bit) 2023.2.0.38.1
    Mapped on: Thu Dec 21 16:41:07 2023

    Design Information

    Command line:   map -i LAB03_Async_rst_syn.udb -pdc
         D:/02_LSCC/09_GSR/Final/LAB03_Sync_rst/Myconstraints.pdc -o
         LAB03_Async_rst_map.udb -mp LAB03_Async_rst.mrp -hierrpt -gui -msgset
         D:/02_LSCC/09_GSR/Final/LAB03_Sync_rst/promote.xml

    Design Summary

       Number of registers:         995 out of 80769 (1%)
          Number of SLICE         registers:  990 out of 79872 (1%)
          Number of PIO Input     registers:    1 out of   299 (<1%)
          Number of PIO Output    registers:    4 out of   299 (1%)
          Number of PIO Tri-State registers:    0 out of   299 (0%)
       Number of LUT4s:            1347 out of 79872 (2%)
          Number used as logic LUT4s:                       1019
          Number used as distributed RAM:                     36 (6 per 16X4 RAM)
          Number used as ripple logic:                       292 (2 per CCU2)
       Number of PIOs used/reserved:   13 out of   299 (4%)
          Number of PIOs reserved:      3 (per sysConfig and/or prohibit constraint)
          Number of PIOs used:         10
            Number of PIOs used for single ended IO:        10
            Number of PIO pairs used for differential IO:    0
            Number allocated to regular speed PIOs:     9 out of  167 (5%)
            Number allocated to high speed PIOs:        1 out of  132 (1%)
       Number of Dedicated IO used for ADC/PCS/PCIE:    0 out of   60 (0%)
       Number of IDDR/ODDR/TDDR functions used:      0 out of   730 (0%)
       Number of IOs using at least one DDR function: 0 (0 differential)
       Number of Block RAMs:          2 out of 208 (1%)
       Number of Large RAMs:          0 out of 7 (0%)
       Number of Logical DSP Functions:
          Number of Pre-Adders (9+9):    0 out of 312 (0%)
          Number of Multipliers (18x18): 0 out of 156 (0%)
             Number of 9X9:        0 (1 18x18 = 2   9x9)
             Number of 18x18:      0 (1 18x18 = 1 18x18)
             Number of 18x36:      0 (2 18x18 = 1 18x36)
             Number of 36x36:      0 (4 18x18 = 1 36x36)
          Number of 54-bit Accumulators: 0 out of 78 (0%)
          Number of 18-bit Registers:    0 out of 312 (0%)
       Number of Physical DSP Components:
          Number of PREADD9:             0 out of 312 (0%)
          Number of MULT9:               0 out of 312 (0%)
          Number of MULT18:              0 out of 156 (0%)
          Number of MULT18X36:           0 out of 78 (0%)
          Number of MULT36:              0 out of 39 (0%)
          Number of ACC54:               0 out of 78 (0%)
          Number of REG18:               0 out of 312 (0%)
       Number of ALUREGs:             0 out of 1 (0%)
       Number of PLLs:                0 out of 4 (0%)
       Number of DDRDLLs:             0 out of 2 (0%)
       Number of DLLDELs:             0 out of 10 (0%)
       Number of DQSs:                0 out of 11 (0%)
       Number of DCSs:                0 out of 2 (0%)
       Number of DCCs:                0 out of 62 (0%)
       Number of PCLKDIVs:            0 out of 2 (0%)
       Number of ECLKDIVs:            0 out of 12 (0%)
       Number of ECLKSYNCs:           0 out of 12 (0%)
       Number of ADC Blocks:          0 out of 1 (0%)
       Number of SGMIICDRs:           0 out of 2 (0%)
       Number of PMUs:                0 out of 1 (0%)
       Number of BNKREF18s:           0 out of 3 (0%)
       Number of BNKREF33s:           0 out of 5 (0%)
       Number of I2CFIFOs:            0 out of 1 (0%)
       Number of Oscillators:         1 out of 1 (100%)
       Number of GSR:                 0 out of 1 (0%)
       Number of Cryptographic Block: 0 out of 1 (0%)
       Number of Config IP:           0 out of 1 (0%)
                     TSALL:           0 out of 1 (0%)
       Number of JTAG:                1 out of 1 (100%)
       Number of SED:                 0 out of 1 (0%)
       Number of PCSs:                0 out of 2 (0%)
       Number of PCIE Link Layers:    0 out of 1 (0%)
       Number of Clocks:  3
          Net jtck: 409 loads, 0 rising, 409 falling (Driver: Pin
         jtaghub_inst.jtagg_u/JTCK)
          Net jtaghub_inst.tck: 1 loads, 1 rising, 0 falling (Driver: Port TCK)
          Net clk150: 530 loads, 530 rising, 0 falling (Driver: Pin
         OSCA001.OSCA_inst/HFCLKOUT)
       Number of Clock Enables:  69
          Net VCC: 2 loads, 0 SLICEs
          Net jtaghub_inst.er1_shift_reg8: 23 loads, 23 SLICEs
          Net ip_enable[0]: 37 loads, 37 SLICEs
          Net jtaghub_inst.JUPDATE: 13 loads, 13 SLICEs
          Net secured_signal_143: 11 loads, 11 SLICEs
          Net secured_signal_152: 3 loads, 3 SLICEs
          Net secured_signal_175: 1 loads, 1 SLICEs
          Net secured_signal_176: 1 loads, 1 SLICEs
          Net secured_signal_188: 10 loads, 10 SLICEs
          Net secured_signal_210: 5 loads, 5 SLICEs
          Net secured_signal_212: 2 loads, 2 SLICEs
          Net secured_signal_216: 3 loads, 3 SLICEs
          Net secured_signal_223: 65 loads, 65 SLICEs
          Net secured_signal_225: 3 loads, 3 SLICEs
          Net secured_signal_228: 3 loads, 3 SLICEs
          Net secured_signal_281: 7 loads, 5 SLICEs
          Net secured_signal_299: 5 loads, 5 SLICEs
          Net secured_signal_300: 5 loads, 5 SLICEs
          Net secured_signal_677: 1 loads, 1 SLICEs
          Net secured_signal_720: 2 loads, 2 SLICEs
          Net secured_signal_726: 20 loads, 20 SLICEs
          Net secured_signal_834: 4 loads, 4 SLICEs
          Net secured_signal_851: 16 loads, 16 SLICEs
          Net secured_signal_986: 16 loads, 16 SLICEs
          Net secured_signal_991: 1 loads, 1 SLICEs
          Net secured_signal_1082: 1 loads, 1 SLICEs
          Net secured_signal_1099: 2 loads, 2 SLICEs
          Net secured_signal_1128: 71 loads, 71 SLICEs
          Net secured_signal_1232: 2 loads, 2 SLICEs
          Net secured_signal_1245: 3 loads, 3 SLICEs
          Net secured_signal_1246: 3 loads, 3 SLICEs
          Net secured_signal_1252: 1 loads, 1 SLICEs
          Net secured_signal_1270: 9 loads, 9 SLICEs
          Net secured_signal_1296: 1 loads, 1 SLICEs
          Net secured_signal_1298: 1 loads, 1 SLICEs
          Net secured_signal_1308: 1 loads, 1 SLICEs
          Net secured_signal_1319: 2 loads, 2 SLICEs
          Net secured_signal_1327: 2 loads, 2 SLICEs
          Net secured_signal_1328: 1 loads, 1 SLICEs
          Net secured_signal_1417: 9 loads, 9 SLICEs
          Net secured_signal_1443: 1 loads, 1 SLICEs
          Net secured_signal_1445: 1 loads, 1 SLICEs
          Net secured_signal_1454: 1 loads, 1 SLICEs
          Net secured_signal_1466: 2 loads, 2 SLICEs
          Net secured_signal_1474: 2 loads, 2 SLICEs
          Net secured_signal_1475: 1 loads, 1 SLICEs
          Net secured_signal_1583: 1 loads, 1 SLICEs
          Net secured_signal_1585: 1 loads, 1 SLICEs
          Net secured_signal_1594: 1 loads, 1 SLICEs
          Net secured_signal_1596: 9 loads, 9 SLICEs
          Net secured_signal_1602: 16 loads, 16 SLICEs
          Net secured_signal_1608: 2 loads, 2 SLICEs
          Net secured_signal_1616: 2 loads, 2 SLICEs
          Net secured_signal_1617: 1 loads, 1 SLICEs
          Net secured_signal_1730: 16 loads, 16 SLICEs
          Net secured_signal_1731: 16 loads, 16 SLICEs
          Net secured_signal_1812: 3 loads, 3 SLICEs
          Net secured_signal_1893: 16 loads, 16 SLICEs
          Net secured_signal_1894: 16 loads, 16 SLICEs
          Net secured_signal_1975: 3 loads, 3 SLICEs
          Net secured_signal_2056: 16 loads, 16 SLICEs
          Net secured_signal_2057: 16 loads, 16 SLICEs
          Net secured_signal_2138: 3 loads, 3 SLICEs
          Net secured_signal_2219: 16 loads, 16 SLICEs
          Net secured_signal_2220: 16 loads, 16 SLICEs
          Net secured_signal_2301: 3 loads, 3 SLICEs
          Net secured_signal_2362: 1 loads, 1 SLICEs
          Net secured_signal_2363: 1 loads, 1 SLICEs
          Net secured_signal_2368: 3 loads, 3 SLICEs
       Number of LSRs:  10
          Net VCC: 4 loads, 0 SLICEs
          Net rsti_1: 36 loads, 36 SLICEs
          Net jrstn: 341 loads, 340 SLICEs
          Net top_reveal_coretop_instance.core0.reset_rvl_n: 524 loads, 524 SLICEs
          Net secured_signal_1376: 1 loads, 1 SLICEs
          Net secured_signal_1377: 1 loads, 1 SLICEs
          Net secured_signal_1524: 1 loads, 1 SLICEs
          Net secured_signal_1525: 1 loads, 1 SLICEs
          Net secured_signal_1683: 1 loads, 1 SLICEs
          Net secured_signal_1684: 1 loads, 1 SLICEs
       Top 10 highest fanout non-clock nets:
          Net top_reveal_coretop_instance.core0.reset_rvl_n: 525 loads
          Net jrstn: 342 loads
          Net top_reveal_coretop_instance.core0.jshift_d1: 106 loads
          Net top_reveal_coretop_instance.core0.addr[4]: 94 loads
          Net top_reveal_coretop_instance.core0.tr_bit_0: 72 loads
          Net secured_signal_1128: 71 loads
          Net secured_signal_223: 65 loads
          Net top_reveal_coretop_instance.core0.addr[0]: 60 loads
          Net top_reveal_coretop_instance.core0.addr[9]: 60 loads
          Net ip_enable[0]: 55 loads

       Number of warnings:  0
       Number of errors:    0

    Design Errors/Warnings

       No errors or warnings present.

    IO (PIO) Attributes

    +---------------------+-----------+-----------+-------+-------+-----------+
    | IO Name             | Direction | Levelmode |  IO   |  IO   | Special   |
    |                     |           |  IO_TYPE  |  REG  |  DDR  | IO Buffer |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | TDI                 | INPUT     |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | TCK                 | INPUT     |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | TMS                 | INPUT     |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | TDO                 | OUTPUT    |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | LED4                | OUTPUT    |           | O     |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | LED3                | OUTPUT    |           | O     |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | LED2                | OUTPUT    |           | O     |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | LED1                | OUTPUT    |           | O     |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | en                  | INPUT     |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | reset               | INPUT     |           | I     |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+

    Removed logic

    Block jtaghub_inst/IP_ENABLE_reg[17].ff_inst undriven or does not drive anything
         - clipped.
    Block jtaghub_inst/IP_ENABLE_reg[16].ff_inst undriven or does not drive anything
         - clipped.
    Block jtaghub_inst/IP_ENABLE_reg[15].ff_inst undriven or does not drive anything
         - clipped.
    Block jtaghub_inst/IP_ENABLE_reg[14].ff_inst undriven or does not drive anything
         - clipped.
    Block jtaghub_inst/IP_ENABLE_reg[13].ff_inst undriven or does not drive anything
         - clipped.
    Block jtaghub_inst/IP_ENABLE_reg[12].ff_inst undriven or does not drive anything
         - clipped.
    Block jtaghub_inst/IP_ENABLE_fast_reg[11].ff_inst undriven or does not drive
         anything - clipped.
    Block jtaghub_inst/IP_ENABLE_reg[11].ff_inst undriven or does not drive anything
         - clipped.
    Block jtaghub_inst/IP_ENABLE_fast_reg[3].ff_inst undriven or does not drive
         anything - clipped.
    Block jtaghub_inst/jtdo2_int_m15_N_2L1_cZ undriven or does not drive anything -
         clipped.
    Block GSR_INST undriven or does not drive anything - clipped.
    Block VCC_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m15_cZ was optimized away.
    Block jtaghub_inst/IP_ENABLE_0_.CN was optimized away.
    Block jtaghub_inst/OBZ_inst_RNO was optimized away.
    Block jtaghub_inst/jtagg_u_RNI1T52 was optimized away.
    Block rsti_1_RNII50D was optimized away.
    Block jtaghub_inst/jtdo2_int_m11_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m11_1_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m8_1_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m11_1_0_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m2_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m2_1_cZ was optimized away.
    Block jtaghub_inst/jtagg_u_RNO_2_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m5_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m5_1_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m2_bm_cZ was optimized away.
    Block jtaghub_inst/jtdo2_int_m5_bm_cZ was optimized away.

    OSC Summary

    OSC 1:                                 Pin/Node Value
      OSC Instance Name:                            OSCA001.OSCA_inst
      Enable High Frequency SDSC:          NODE     VCC
      High Frequency Output:               NODE     clk150
      Low Frequency Output:                         NONE
      SDC Output:                                   NONE
      High Frequency DIV:                           3

    ASIC Components

    Instance Name: jtaghub_inst/jtagg_u
             Type: CONFIG_JTAG_CORE
    Instance Name: secured_comp_287
             Type: EBR_CORE
    Instance Name: secured_comp_288
             Type: EBR_CORE
    Instance Name: OSCA001.OSCA_inst
             Type: OSC_CORE

    Constraint Summary

       Total number of constraints: 19
       Total number of constraints dropped: 0

    Run Time and Memory Usage

       Total CPU Time: 0 secs
       Total REAL Time: 6 secs
       Peak Memory Usage: 665 MB
    Checksum -- map: 821725cadb6eeba8ceb2e7bf1070fd238f3f7b48
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995
         AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent
         Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems
         All rights reserved.
    Copyright (c) 2002-2023 Lattice Semiconductor
         Corporation,  All rights reserved.